**Asc3QtKdClient Quick Reference**

**Keyboard shortcuts**

**Key** **Function**

|  |  |
| --- | --- |
| Enter | Enter |
| “f”, “\*” | Spec Func |
| “m”, Home | Main Menu |
| Escape, End | Sub Menu |
| “.”, Delete, “c” | Clear |
| “+”, ”s” | Status |
| “h”, ”/” | Help |
| “d”,”-“ | Next Data |
| Page Down | Next Screen |
| Page Up | Next Page |
| Left Arrow | Left Arrow\* |
| Right Arrow | Right Arrow\* |
| Up Arrow | Up Arrow\* |
| Down Arrow | Down Arrow\* |
| Space | “0” (Toggle on/off) |

\*Note: The arrow keys may only work if other buttons on the display haven’t been clicked. If any button has a dotted line around it on the display, the arrow keys will only move between the display buttons, rather than move around the controller screen. Clicking the “Connect” button will clear this condition and allow you to navigate the controller screen with the arrow keys again.

**Rotary Dial**

The rotary dial at the top-right of the display changes the polling rate of the program. A lower value will provide a faster refresh of the controller screen, but may cause problems with high latency controllers like 2070s.

**Connection**

When entering an IP address for the connection, the tab key allows movement from one field to the next, and pressing the enter key will connect to the controller.